
; Windows USB CDC ACM Setup File
; Copyright (c) 2000 Microsoft Corporation
; Copyright (C) 2010 Bluegiga

[Version] 
Signature="$Windows NT$" 
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318} 
Provider=%MFGNAME% 
LayoutFile=layout.inf
CatalogFile=%MFGFILENAME%.cat
DriverVer=11/15/2007,5.1.2600.0

[Manufacturer] 
%MFGNAME%=DeviceList, NTamd64

[DestinationDirs] 
DefaultDestDir=12 


;------------------------------------------------------------------------------
;  Windows 2000/XP/Vista-32bit Sections
;------------------------------------------------------------------------------

[DriverInstall.nt] 
include=mdmcpq.inf
CopyFiles=DriverCopyFiles.nt
AddReg=DriverInstall.nt.AddReg 

[DriverCopyFiles.nt]
usbser.sys,,,0x20

[DriverInstall.nt.AddReg] 
HKR,,DevLoader,,*ntkern 
HKR,,NTMPDriver,,%DRIVERFILENAME%.sys 
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider" 

[DriverInstall.nt.Services] 
AddService=usbser, 0x00000002, DriverService.nt

[DriverService.nt] 
DisplayName=%SERVICE% 
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\%DRIVERFILENAME%.sys 

;------------------------------------------------------------------------------
;  Vista-64bit Sections
;------------------------------------------------------------------------------

[DriverInstall.NTamd64] 
include=mdmcpq.inf
CopyFiles=DriverCopyFiles.NTamd64
AddReg=DriverInstall.NTamd64.AddReg 

[DriverCopyFiles.NTamd64]
%DRIVERFILENAME%.sys,,,0x20

[DriverInstall.NTamd64.AddReg] 
HKR,,DevLoader,,*ntkern 
HKR,,NTMPDriver,,%DRIVERFILENAME%.sys 
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider" 

[DriverInstall.NTamd64.Services] 
AddService=usbser, 0x00000002, DriverService.NTamd64

[DriverService.NTamd64] 
DisplayName=%SERVICE% 
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\%DRIVERFILENAME%.sys 


;------------------------------------------------------------------------------
;  Vendor and Product ID Definitions
;------------------------------------------------------------------------------
; When developing your USB device, the VID and PID used in the PC side
; application program and the firmware on the microcontroller must match.
; Modify the below line to use your VID and PID.  Use the format as shown below.
; Note: One INF file can be used for multiple devices with different VID and PIDs.
; For each supported device, append ",USB\VID_xxxx&PID_yyyy" to the end of the line.
;------------------------------------------------------------------------------
[SourceDisksFiles]
[SourceDisksNames]
[DeviceList]
%DESCRIPTION%=DriverInstall, USB\VID_2458&PID_0001 

[DeviceList.NTamd64] 
%DESCRIPTION%=DriverInstall, USB\VID_2458&PID_0001


;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------
;Modify these strings to customize your device
;------------------------------------------------------------------------------
[Strings]
MFGFILENAME="Bluegiga Bluetooth Low Energy"
DRIVERFILENAME ="usbser"
MFGNAME="Bluegiga"
INSTDISK="Bluegiga, Installation Disc"
DESCRIPTION="Bluegiga Bluetooth Low Energy"
SERVICE="USB Bluegiga Bluetooth Low Energy RS-232 Emulation Driver"


